Annex C
Technical Proposal
	Name of Participant:
	[Insert Name of Participant]
	Date:
	

	CFB reference:
	No. CFB/MDA/EQ3/SS/14/2026



Where a descriptive response is requested, failure to provide the same will be viewed as non-responsive.
The bidder's offer should be organized to follow this format of the Technical Proposal. The participant must describe the exact type of each offered item and provide relevant product information or visualization for each item. The quality of the goods offered may exceed the minimum technical requirements of this CFB. 

	No
	MINIMUM REQUIREMENTS
	Technical specification
	OFFER 1
	OFFER 2
	OFFER 3

	
	
	
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin

	1
	Secure storage – large safe with key lock
	Large safe with key lock for protected storage of sensitive materials, documentation and selected assets; external dimensions approximately 1950 x 930 x 520 mm (H x W x D); internal dimensions approximately 1800 x 820 x 420 mm; double-wall steel body with fire-resistant insulating fill between the walls; burglary resistance minimum Grade S2 per EN 14450; fire resistance minimum 30 minutes; door thickness minimum 60 mm; multi-point locking mechanism with minimum 4 locking bolts of minimum 20 mm diameter; door opening angle up to 180° via external hinges; high-security double-bit key lock supplied with two keys and handle; adjustable interior shelving, maximum shelf load minimum 40 kg; floor/wall anchoring points; complete with manufacturer's test/compliance certificate and user documentation in English.
	
	
	

	2
	Secure storage – large safe with electronic lock
	Large safe with electronic lock for protected storage and controlled access to sensitive contents; external dimensions approximately 1950 x 930 x 520 mm (H x W x D); internal dimensions approximately 1800 x 820 x 420 mm; double-wall steel body with fire-resistant insulating fill between the walls; burglary resistance minimum Grade S2 per EN 14450; fire resistance minimum 30 minutes; door thickness minimum 60 mm; multi-point locking mechanism with minimum 4 locking bolts of minimum 20 mm diameter; door opening angle up to 180° via external hinges; electronic combination lock with digital keypad, minimum 6-digit user code and audible/visual access indication, battery-powered with low-battery warning; adjustable interior shelving, maximum shelf load minimum 40 kg; floor/wall anchoring points; complete with manufacturer's test/compliance certificate and user documentation in English.
	
	
	

	3
	Secure storage – large safe with key + electronic lock
	Large safe with combined key and electronic locking for increased security and dual-control access; external dimensions approximately 1950 x 930 x 520 mm (H x W x D); internal dimensions approximately 1800 x 820 x 420 mm; double-wall steel body with fire-resistant insulating fill between the walls; burglary resistance minimum Grade S2 per EN 14450; fire resistance minimum 30 minutes; door thickness minimum 60 mm; multi-point locking mechanism with minimum 4 locking bolts of minimum 20 mm diameter; door opening angle up to 180° via external hinges; combined locking comprising a high-security double-bit key lock (two keys) plus an independent electronic combination lock with digital keypad; adjustable interior shelving, maximum shelf load minimum 40 kg; floor/wall anchoring points; complete with manufacturer's test/compliance certificate and user documentation in English.
	
	
	

	4
	Secure storage – metal safe with key lock
	Metal safe for distributed secure storage at lower-tier facilities or working areas, key lock; external dimensions approximately 630 x 440 x 355 mm (H x W x D); internal dimensions approximately 500 x 434 x 301 mm; internal capacity approximately 66 litres, including a separate small lockable compartment (approx. 13 litres) for cash/valuables; burglary resistance minimum Grade S1 per EN 14450; three-way locking bolt mechanism with integrated relocker protecting against drilling attacks; high-security double-bit key lock supplied with two keys; minimum 1 adjustable interior shelf; floor/wall anchoring points/holes; complete with manufacturer's test/compliance certificate and user documentation in English.
	
	
	

	5
	Secure storage – metal safe with electronic lock
	Metal safe for distributed protected storage and accountability at lower-tier facilities or working areas, electronic lock; external dimensions approximately 630 x 440 x 355 mm (H x W x D); internal dimensions approximately 500 x 434 x 301 mm; internal capacity approximately 66 litres, including a separate small lockable compartment (approx. 13 litres) for cash/valuables; burglary resistance minimum Grade S1 per EN 14450; three-way locking bolt mechanism with integrated relocker protecting against drilling attacks; electronic combination lock with digital keypad, minimum 6-digit user code and audible/visual access indication, battery-powered with low-battery warning; minimum 1 adjustable interior shelf; floor/wall anchoring points/holes; complete with manufacturer's test/compliance certificate and user documentation in English.
	
	
	



We attach the following: 
a) Technical information (if necessary) – ……. (number of pages); 

Authorized signature: ___________________________ 
(Name of authorized signatory)
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