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Where a descriptive response is requested, failure to provide the same will be viewed as non-responsive.
The bidder's offer should be organized to follow this format of the Technical Proposal. The participant must describe the exact type of each offered item and provide relevant product information or visualization for each item. The quality of the goods offered may exceed the minimum technical requirements of this CFB. 

	No
	MINIMUM REQUIREMENTS
	Technical specification
	OFFER 1
	OFFER 2
	OFFER 3

	
	
	
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin

	1
	Field power generation – diesel generator set
	Portable diesel generator set for field/backup power at temporary command posts, training areas and dispersed activities when grid supply is unavailable or degraded; single-cylinder, 4-stroke, air-cooled, direct-injection diesel engine, displacement ≥ 400 cm³; rated (continuous) output ≥ 6.0 kW, maximum output ≥ 6.5 kW; output 230V AC, single-phase, 50Hz ±2%; protection rating minimum IP23; manual start (recoil/key), electric start considered an advantage; fuel tank minimum 12 L, providing no less than 5 hours autonomy at rated load; minimum 2× 230V output sockets with overload circuit-breaker protection and automatic low-oil-level shutdown; open-frame or skid-mounted design with carrying/lifting points for field portability; CE marking or equivalent recognized conformity marking; complete with tool kit, funnel and user manual/documentation in English.
	
	
	

	2
	Field power generation – petrol generator set
	Portable petrol (gasoline) generator set complementing the diesel units for smaller loads, auxiliary field tasks and flexible deployment; single-cylinder, 4-stroke, air-cooled, OHV petrol engine, displacement ≥ 200 cm³ (≥ 6 HP); rated (continuous) output ≥ 2.7 kW, maximum output ≥ 3.0 kW; output 230V AC, single-phase, 50Hz ±2%, with Automatic Voltage Regulator (AVR); rated current ≥ 11 A; auxiliary 12V DC output for battery charging; manual recoil start; fuel tank minimum 14 L, providing no less than 8 hours autonomy at rated load; minimum 2× 230V output sockets plus 1× 12V DC output, with overload circuit-breaker protection; wheel and folding-handle transport kit for portability; CE marking or equivalent recognized conformity marking; complete with tool kit and user manual/documentation in English.
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