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Technical Proposal
	Name of Participant:
	[Insert Name of Participant]
	Date:
	

	CFB reference:
	No. CFB/MDA/EQ3/FB /17/2026


Where a descriptive response is requested, failure to provide the same will be viewed as non-responsive.
The bidder's offer should be organized to follow this format of the Technical Proposal. The participant must describe the exact type of each offered item and provide relevant product information or visualization for each item. The quality of the goods offered may exceed the minimum technical requirements of this CFB. 

	No
	MINIMUM REQUIREMENTS
	Technical specification
	OFFER 1
	OFFER 2
	OFFER 3

	
	
	
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin
	Brand / Model / PN / Origin

	1
	Deployable command-post/classroom furniture – folding table
	Foldable table for rapidly establishing temporary briefing, planning and training areas; rectangular tabletop, minimum 150 x 70 cm (L x W); tabletop material: high-pressure laminate (HPL) or water-resistant coated board, wipeable surface; frame: powder-coated tubular steel with folding leg mechanism for compact storage and transport; static load capacity minimum 80 kg evenly distributed; standard working height approximately 74 cm; stackable for storage; complete with user/assembly instructions.
	
	
	

	2
	Deployable command-post/classroom furniture – folding chair
	Foldable chair supporting temporary command-post, training and coordination functions; frame: powder-coated tubular steel with folding mechanism for compact storage and transport; seat and backrest: weather- and wear-resistant polypropylene or equivalent material; static load capacity minimum 110 kg; stackable for storage; lightweight and portable design; complete with user/assembly instructions.
	
	
	

	3
	Planning and briefing aids – large-format magnetic board
	Large-format magnetic whiteboard / display board for planning, instruction, and coordination sessions; diagonal/format minimum 78" (approx. 198 cm) or equivalent large working surface; magnetic steel writing surface with scratch- and stain-resistant coating; aluminium frame; mobile stand with lockable castor wheels or adjustable easel-type support enabling repositioning between briefing/planning areas; complete with pen tray and mounting/assembly hardware.
	
	
	

	4
	Planning and briefing aids – magnetic board 120x180cm
	Magnetic whiteboard for distributed working groups, planning cells and instructional use; size 120 x 180 cm (H x W) or equivalent; magnetic steel writing surface with scratch- and stain-resistant coating; aluminium frame with rounded corners; wall-mountable with complete mounting hardware; complete with pen tray.
	
	
	

	5
	Field audio/public address – portable wireless speaker
	Portable wireless speaker for field coordination, announcements and training support; multi-driver 2-way bass-reflex design (tweeters and woofers) delivering room-filling/outdoor-capable sound output; nominal amplifier output minimum 300 W; Bluetooth wireless connectivity version 5.0 or higher; wired inputs: minimum one 3.5 mm auxiliary/microphone input; built-in rechargeable battery providing minimum 15 hours of continuous playback, with AC mains charging/operation; splash resistance minimum IPX4; integrated carrying handle and transport wheels; complete with power cable and user documentation.
	
	
	

	6
	Field audio/public address – megaphone
	Megaphone for immediate field communication, marshalling and local crowd/personnel control; amplifier output minimum 25 W RMS (minimum 80 W peak); effective range minimum 600 m in open field; functions: voice amplification, siren and whistle/alarm tone; battery-powered, weatherproof housing including battery compartment; integrated or attachable handheld microphone; adjustable volume control; carrying strap included; complete with user documentation.
	
	
	

	7
	Visual display – 55" smart TV
	Large flat-panel display for presentations, COP (Common Operational Picture) display or instructional use; screen size minimum 55" (approx. 140 cm) diagonal; resolution minimum 3840 x 2160 (4K UHD); minimum 3x HDMI inputs and 2x USB ports; built-in smart TV platform with Wi-Fi and Ethernet connectivity for network/content display; wall-mount compatible (VESA standard) and supplied with table-top stand; complete with remote control and user documentation in English.
	
	
	

	8
	Visual display support – mobile TV floor stand
	Mobile TV stand enabling flexible deployment of the visual display in briefing or temporary command-post environments; compatible with screens from 37" up to at least 70"; VESA mounting compatibility up to 600 x 400 mm; height-adjustable or fixed-height aluminium/steel construction with stable weighted base; lockable castor wheels for mobility and repositioning; rated load capacity minimum 40 kg; complete with mounting hardware and assembly instructions.
	
	
	



We attach the following: 
a) Technical information (if necessary) – ……. (number of pages); 

Authorized signature: ___________________________ 
(Name of authorized signatory)
 
Functional Title: ___________________



