

CRISIS MANAGEMENT AND DISASTER RESPONSE CENTRE OF EXCELLENCE

ЦЕНТЪР ЗА ИЗСЛЕДВАНЕ, ИЗГРАЖДАНЕ И УСЪВЪРШЕНСТВАНЕ НА СПОСОБНОСТИ НА НАТО ЗА УПРАВЛЕНИЕ НА КРИЗИ И РЕАГИРАНЕ ПРИ БЕДСТВИЯ

**OUTDATED EQUIPMENT - FOR SALE /TECHNICAL SPECIFICATIONS/**

**ИЗЛЯЗЛО ОТ УПОТРЕБА ОБОРУДВАНЕ - ЗА ПРОДАЖБА /ТЕХНИЧЕСКИ ДАННИ/**

**Network Printer – Konica Minolta Bizhub C 25 specifications:**

|  |  |
| --- | --- |
| **Type** | Desk top Full-Colour Printer/Copier/Scanner |
| **Colour Support** | Full colour |
| **Copy Resolution** | 600dpi × 600dpi |
| **Scanning Resolution** | 600dpi × 600dpi |
| **Print Resolution** | 600dpi × 600dpi × 3bit |
| **Gradation** | 256 colour shades per pixel (8-bit) |
| **Memory Capacity** | **Copy** | 128MB (Shared witd copy, s can and fax) (Std/Max) |
| **Print** | 256MB (Std) / 512MB (Max)) |
| **HDD** | 40GB (optional) (Printer only) |
| **Original Type** | Sheets, Books, Objects |
| **Max. Original Size** | A4 or 8.5″ × 14″ (ADF only) |
| **Output Size** | **Tray 1 (Standard)** **(Multiple Bypass Tray)** | A4, A5, B5, A6, B6, 16K 4″ × 6″, 5.5″ × 8.5″, 8.5″ × 11″, 8.5″ × 14″ |
| **Tray 2 (Standard)** **(Universal Tray)** | A4, A5, B5, A6, B6, 16K 4″ × 6″, 5.5″ × 8.5″, 8.5″ × 11″ |
| **Tray 3 (Optional)** **(Universal Tray)** | A4, B5 8.5″ × 11″, 8.5″ × 14″ |
| **Image Loss** | **Copy** | Max. 4.0 mm for Top/bottom/right/left edge |
| **Print** | Max. 4.2 mm for Top/bottom/right/left edge |
| **Warm-Up Time (23ºC, std. voltage)** | 38 sec. or less (May vary depending on tde operating environment and usage.) |
| **First Copy Time** | **Colour/B&W** | 16.0 sec. or less/11. 0 sec. or less (600 × 300 dpi, fastest speed) (A4) |
| **First Print Time** | **Colour/B&W** | 16.0 sec. or less (A4) |
| **Copy/ Print Speed (continuous)** | **Colour/B&W** | 24 cpm (ppm) (A4) |
| **Copy Magnification** | **Fixed Same Magnification** | 1:1± 1. 0% or less |
|  | **Scaling Up** | 1:1.15 / 1.41 / 2.00 / 4.00 |
| **Scaling Down** | 1:0.86 / 0.70 / 0.50 / 0.25 |
| **Zoom** | **Flatbed** | 25 to 400%, 1% increments |
| **ADF** | 25 to 400%, 1% increments |
| **Paper Capacity** | **Standard** | 100-sheet multiple bypass tray, 250-sheet universal tray |
| **Max.** | 850 sheets (total, witd options) |
| **Paper Weight** | 60 to 210 g /m2 |
| **Multiple Print** | 1 to 99 sheets |
| **Power Requirement** | 220 to 240 V (50 to 60 Hz) |
| **Max. Power Consumption** | 1.1 kW or less |
| **Dimensions [W] × [D] × [H]** | 447 mm × 558 mm × 490 mm (17-1/2″ × 22″ × 19-1/4″) |
| **Weight** | 32kg (70-1/2lb) |